# IP Camera

## Smartphone -ready colour night/day

## network camera with pan, tilt and zoom

**DYN-627**



# Specification

* Product type：IP camera
* Operation system：Embedded operating system
* Web protocol：TCP/IP, UDP/IP, HTTP, SMTP, FTP, DHCP, DDNS, UPNP, NTP, RTSP, ONVIF
* LAN port：10Base-T/100Base-TX
* Wifi：802.11 b/g/n
* Resolution：720P, 640\*360, 320\*180
* Compression mode：H.264/M-JPEG
* Max frame rate：30fps
* Lens：f=4mm, F=1.2
* Min. illumination：IR on, 0 Lux
* Electronic shutter：1/50s(1/60s)-1/100,000 s
* SNR：48db
* Safety performance：Three levels of user rights
* Install mode：ceiling-mounted
* Other performance：PC software,support for Microsoft Windows 98/2000/XP/Vista/Windows 7/Mac OS,And the Internet Explorer6.1 and above version or browser compatibility, Firefox, etc., provide iSmartViewPro client software
* Power supply：DC 12V
* Sensor：CMOS Sensor
* IP camera performance：Support video control, Two-way voice talkback, motion detection, external alarm(sends information to alarm the server by Email, FTP);Manufacturers provide free DDNS, and has been written into equipment; 10pcs IR LEDs, 8meters effectively; Platform level angle 350°, 120 °vertical angle; automatically control through the photoresistor;
* Audio input：None
* Audio output：None
* Alarm in：None
* Alarm out：None
* Power consumption：Power<8W
* Body size：130\*130\*100mm
* Product weight：0.36kg
* Environment temperature：-10℃--50℃℃
* Environment humidity：below 85% RH