### 10 Way Vertically Mounted Schuko Plug PDU - 16A Schuko Sockets (PDU-10WS-V-SCH-SCH)



# **Description:**

The LMS Power**PDU-10WS-V-SCH-SCH**is a high-quality vertically mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the mounting brackets of data, telecom and server cabinets.

A must-have accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch, high-load standardised 16 A rated Schuko power input plug connected to Schuko output power sockets.

# **Key Features:**

**Standard Schuko power outlets for your appliances

   Standardised Schuko 16 Amp power plug**   **1U vertically mounted attaches to internal profiles**

**Neon On/Off Rocker switch to prevent accidental turn off**

**Backed up by LMS Power's exclusive 3-year warranty**

# **Applications:**

# Create instant power feeds to your data, telecom, server and H/VAC

# Provide effective power for cabinet cooling fans, UPS systems

# Ideal as stand-alone trailing sockets outside the cabinet

# **Product Code:**

Part Number: PDU-10WS-V-SCH-SCH

EAN: 8400800033277

Weight: 1.7Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty

Chassis                    1U vertical PDU with mounting brackets

Output Sockets     10 Schuko Sockets

Power Input            Standardised Schuko Plug

Flex Length             1.8 metres (approx)

Power Control        On/Off Rocker Switch (illuminated)

Power Rating          4000 Watts (approx) Surge Protected

# **Supplied With:**

PDU-10WS-V-SCH-SCH   10 Way Vertical PDU

Cabinet brackets (Fitted)

*\* Specifications and product design are subject to change. E&OE.*

Looking for highperformance power distribution using the industry standard Schuko(tm) fitment? The newly developed LMS Data 16A heavy-duty horizontal, rack-mount PDU is ideal for high-loading device requirements including server, network and other industrial-type equipment functions such as broadcast and HVAC applications, plus ideal for EU/European AC power applications. Combining a fully certified Schuko(tm) 16A plug input combined with a compatible heavy load power flex means you can be assured this LMS Data PDU can work without problems, 24/7. Furthermore, incorporated onto the horizontal form-factor is standard Schuko(tm) sockets, 6 in total, allowing for safe and secure electrical power feeds to your high power appliances and devices. Robust in design, with an integral neon illuminated rocker switch for assured functionality, the LMS Data PDU is designed to deliver maximum electrical power today and tomorrow.

# **specifications:**

Horizontal high-performance Power Distribution Unit

Industry standard Schuko(tm) power outlets (8 outlets)

Industry-standard Schuko(tm) male EU fitted plug

Robust, black aluminium design for industrial use

Neon on/off power switch for assured control and safety

1.8 metre (approx.) power cordage

Ideal for data, telecom, broadcast and HVAC applications