### 10 Way Vertically Mounted Rackmount 16A Commando PDU - UK Sockets (PDU-10WS-V-16CMDO)



# **Description:**

The LMS Power **PDU-10WS-V-16CMDO** is a high-quality vertically mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.

A must-have accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, 16-Amp rated
heavy duty Commando power input plug, ideal for industrial usage.

# **Key Features:**

Standard UK 3-Pin power outlets for your appliances

HD Commando Plug for industrial applications

1U high means the PDU can fit into the smallest cabinet

Neon On/Off Rocker switch to prevent accidental turn off

Backed up by LMS Power's exclusive 3-year warranty

# **Applications:**

Create instant power feeds to your data, telecom or server cabinets

Provide effective power for cabinet cooling fans, UPS systems

Ideal as stand-alone trailing sockets outside the cabinet

# **Product Code:**

Part Number: PDU-10WS-V-16CMDO

EAN: 8400800032010

Weight: 1.5Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty

Chassis                   1U vertical mount with mounting brackets

Output Sockets      10 UK 3-PIN Sockets

Power Input            Fitted 16-Amp HD Commando Plug

Flex Length             1.8 metres (approx)

Power Control        On/Off Rocker Switch (illuminated)

Power Rating          4000 Watts (approx)

# **Supplied With:**

PDU-10WS-V-16CMDO    10 Way Vertical PDU

19-inch cabinet brackets (Fitted)

*\* Specifications and product design are subject to change. E&OE.*

Looking for highperformance power distribution for your heavily loaded systems? The newly developed LMS Data 16A heavy-duty vertical PDU is ideal for highloading device requirements including server, network and other industrial-type equipment functions such as broadcast and HVAC applications. Combining a fully certified commando type 16A plug input combined with a compatible heavy load power flex means you can be assured this LMS Data PDU can work without problems, 24/7. Furthermore, incorporated onto the vertical form-factor are industry standard UK 3-pin sockets, ideal for data, telco and broadcast equipment. Robust in design, with an integral neon illuminated rocker switch for assured functionality, the LMS Data PDU is designed to deliver maximum electrical power today and tomorrow.

# **specifications:**

Vertical, high-performance Power Distribution Unit (PDU)

Heavy-load 16A Commando style 3-pin plug

Compatible, heavy-load power cable

10x UK style output power sockets

Robust, black aluminium design for industrial use

Neon on/off power switch for assured control

Maximum power rating - 4000W

2.0 metre (approx.) power cordage

Ideal for data, telecom, broadcast and HVAC applications