### 16 Way Horizontally Mounted Rackmount IEC 14 Plug PDU - IEC 13 Sockets (PDU-16W-H-IEC-IEC)



# **Description:**

# The LMS Power PDU-16W-H-IEC-IEC is a high-quality horizontally mounted PDU (Power Distribution Unit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.

# A must-have accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

# Robust, alloy design complete with rackmount brackets fitted with a standardised IEC 13 power outlets, the PDU being fitted with a standardised IEC 14 Plug.

# **Key Features:**

**Standard IEC 13 power outlets for your appliances**

**Standardised IEC 14 power plug**

**1U horizontally mounted attaches to internal profiles**

**Backed up by LMS Power's exclusive 3-year warranty**

# **Applications:**

Create instant power feeds to your data, telecom or server cabinets

Provide effective power for cabinet cooling fans, UPS systems

Ideal as stand-alone trailing sockets outside the cabinet

# **Product Code:**

Part Number: PDU-16W-H-IEC-IEC

EAN: 8400800036216

Weight: 1.7Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty

Chassis                    1U horizontally PDU with mounting brackets

Output Sockets     16 IEC 13 Sockets

Power Input            Standardised IEC 14 Plug

Flex Length             2 metres (approx)

Power Rating          4000 Watts (approx) Surge Protected

# **Supplied With:**

PDU-16W-H-IEC-IEC    16 Way Horizontal PDU

Cabinet brackets (Fitted)
*\* Specifications and product design are subject to change. E&OE.*

Looking for highperformance power distribution for your heavily loaded systems? The newly developed LMS Data 10A heavy-duty horizontal PDU using the modular IEC-14 input connector which is ideal for many device requirements including server, network and other industrial-type equipment functions such as broadcast and HVAC applications. Combining a fully certified IEC-14 plug input combined with a compatible heavy load power flex means you can be assured this LMS Data PDU can work without problems, 24/7. Furthermore, incorporated onto the horizontal form-factor are industry standard IEC-13 sockets, ideal for data, telco and broadcast equipment with the added benefit of integral electrical surge protection. Robust in design, with an integral neon illuminated rocker switch for assured functionality, the LMS Data PDU is designed to deliver maximum electrical power today and tomorrow.

# **specifications:**

Horizontal, high-density Power Distribution Unit (PDU)

Modular 10A IEC-14 style plug format

Compatible, heavy-load power cable

12x IEC-13 output power sockets

Robust, black aluminium design for industrial use

Neon on/off power switch for assured control

Maximum power rating - 4000W

2.0 metre (approx.) power cordage

Ideal for data, telecom, broadcast and HVAC applications