### 8 Way Vertically Mounted Rackmount 32A Commando PDU - UK Sockets (PDU-8WS-V-32CMDO)

### 

# **Description:**

The LMS Power **PDU-8WS-V-32CMDO** is a high-quality vertically mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.   
  
A must-have accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.  
  
Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, 32-Amp rated extra heavy duty Commando power input plug, ideal for industrial usage.

# **Key Features:**

Standard UK 3-Pin power outlets for your appliances  
  
Extra HD 32 Amp Commando Plug for industrial applications  
  
1U high means the PDU can fit into the smallest cabinet  
  
Neon On/Off Rocker switch to prevent accidental turn off   
  
Backed up by LMS Power's exclusive 3-year warranty

# **Product Code:**

Part Number: PDU-8WS-V-32CMDO

EAN: 84008000361627

Weight: 1.6Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty  
                         
Chassis                  1U vertical mount with mounting brackets   
  
Output Sockets     8 UK 3-PIN Sockets

Power Input            Fitted 32-Amp HD Commando Plug  
  
Flex Length             1.8 metres (approx)  
  
Power Control        On/Off Rocker Switch (illuminated)  
  
Power Rating          4000 Watts (approx)

# **Supplied With:**

PDU-8WS-V-32CMDO    8 Way Vertical PDU  
  
19-inch cabinet brackets (Fitted)  
*\* Specifications and product design are subject to change. E&OE.*

Looking for high-performance power distribution for your heavily loaded systems using the industry standard 32 amp commando plug power input? The newly developed LMS Data 32A heavy-duty vertical PDU is ideal for high-loading device requirements including server, network and other industrial-type equipment functions such as broadcast and HVAC applications. Combining a fully certified commando type 32A plug input, combined with a compatible heavy load power flex means you can be assured this LMS Data PDU can work without problems, 24/7. Ideal for vertical placement in wide range of data, server and broadcast cabinets that need a higher load equipment environments. Robust in design, with an integral illuminated power input status, the LMS Data PDU is designed to deliver maximum electrical power today and tomorrow.

# **specifications:**

Vertical, high-performance Power Distribution Unit (PDU)

Heavy-load 32A Commando style 3-pin plug

Compatible, heavy-load power cable

x8 UK style output power sockets - Non surge protection

Robust, black aluminium design for industrial use

Illuminated power input light for assured power status

Maximum power rating - 4000W nominal

1.8 metre (approx.) power cordage - 3x4mm2 dimensions

Ideal for data, telecom, broadcast and HVAC applications