# 

**XQD and SD Card Reader**

Professional-Class XQD"M, SDTM and USB3 Adapter



# Descrption:

# XQDTM is the latest in high-performance, high-capacity memory cards featured in the latest DSLR and mirror-less cameras from NikonTM, SonyTM, Phase OneTM and is sure to be the stable diet of still image and 4K video storage for future imaging devices.

# Using the high-speed Type-C interface, not only is a XQDTM reader included but also a SDTMHC slot for UHS-I/II memory cards. Included is a standard USB3.0 port which allows connection to almost any other USB device, such as flash drives, storage etc and can be used simultaneously with the other onboard memory card slots.

# Features:

* XQDTM transfer speeds up to 4-Gbits/s, 500Mbps
* Ultra-fast RAW, JPG, 4K or higher file copies from memory cards
* SonyTM, LexarTM and other compatible XQDTM support
* SDTMHC reader, compatible with UHS-I/II SDTM cards
* USB3.0 port for connection to almost all USB devices
* Type-C connectivity - self-powered and Plug n' Play

# Specifications

* Material: ASB Housing
* Cable Length: 11.5cm
* Color: black
* Input：type c
* Output：SD card/XQD card/USB
* Speed：1G takes 2 minutes and 30 second normally
* Quality：High and stable
* Certificate: CE FCC ROHS
* Operating Temperature:0℃ to +45℃
* Operating Humidity:10%0 to 85 % RH
* Storage Temperature : -10℃ to +55℃
* Storage Humidity: 5% to 90 % RH

# Product Code:

Part number: C-TC-CR-USB3

Barcode: 8400800036568

Size: 45mm x 6mm x 14mm

