### 10 Way Vertically Mounted Rackmount IEC PDU - UK Sockets (PDU-10WS-V-UK-IEC)



# **Description:**

The LMS Power **PDU-10WS-V-UK-IEC** is a high-quality vertically mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.

A must-have accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, certified IEC-14 power input plug.

# **Key Features:**

Standard UK 3-Pin power outlets for your appliances

Certified IEC-14 power input plug

1U high means the PDU can fit into the smallest cabinet

Neon On/Off Rocker switch to prevent accidental turn off

Backed up by LMS Power's exclusive 3-year warranty

# **Applications:**

Create instant power feeds to your data, telecom or server cabinets

Provide effective power for cabinet cooling fans, UPS systems

Ideal as stand-alone trailing sockets outside the cabinet

# **Product Code:**

Part Number: PDU-10WS-V-UK-IEC

EAN: 8400800036124

Weight: 1.1Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty

Chassis                   1U vertical mount with mounting brackets

Output Sockets      10 UK 3-PIN Sockets

Power Input            Fitted IEC-14 Plug

Flex Length             1.8 metres (approx)

Power Control        On/Off Rocker Switch (illuminated)

Power Rating          4000 Watts (approx)

# **Supplied With:**

PDU-10WS-V-UK-IEC   10 Way Vertical PDU

19-inch cabinet brackets (Fitted)

*\* Specifications and product design are subject to change. E&OE.*

Looking for highperformance power distribution for your heavily loaded systems? The newly developed LMS Data 10A heavy-duty vertical PDU using the modular IEC-14 input connector which is ideal for many device requirements including server, network and other industrial-type equipment functions such as broadcast and HVAC applications. Combining a fully certified IEC-14 plug input combined with a compatible heavy load power flex means you can be assured this LMS Data PDU can work without problems, 24/7. Furthermore, incorporated onto the vertical form-factor are industry standard UK sockets, ideal for data, telco and broadcast equipment with the added benefit of integral electrical surge protection. Robust in design, with an integral neon illuminated rocker switch for assured functionality, the LMS Data PDU is designed to deliver maximum electrical power today and tomorrow.

# **specifications:**

Vertical, high-density Power Distribution Unit (PDU)

Modular 10A IEC-14 style plug format

Compatible, heavy-load power cable

10x UK output power sockets

Robust, black aluminium design for industrial use

Neon on/off power switch for assured control

Maximum power rating - 4000W

2.0 metre (approx.) power cordage

Ideal for data, telecom, broadcast and HVAC applications