### 12 Way Vertically Mounted Surge Protected Rackmount PDU - UK Sockets (PDU-12WS-V-SP-1U)



# **Description:**

The LMS Power **PDU-12WS-V-SP-1U** is a high-quality surge protected, vertically mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.   
  
Providing piece-of-mind of integral electrical surge protection against common power surges and electrical spikes to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.  
  
Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, BSI-fitted  
13 Amp UK plug.

# **Key Features:**

# **Standard UK 3-Pin power outlets for your appliances**

# **Built-in surge protection for critical device protection**

# **1U vertically mounted attaches to internal profiles**

# **Neon On/Off Rocker switch to prevent accidental turn off**

# **Backed up by LMS Power's exclusive 3-year warranty**

# **Applications:**

Create instant power feeds to your data, telecom or server cabinets  
  
Provide effective power for cabinet cooling fans, UPS systems  
  
Ideal as stand-alone trailing sockets outside the cabinet

# **Product Code:**

Part Number: PDU-12WS-V-SP-1U  
  
EAN: 8400800021038

Weight: 1.6Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty  
                         
Chassis                   1U vertical PDU with mounting brackets   
  
Output Sockets      12 UK 3-PIN Sockets

Power Input            Fitted UK 3PIN BSI Plug 13 Amp  
  
Flex Length             1.8 metres (approx)  
  
Power Control        On/Off Rocker Switch (illuminated)  
  
Power Rating          4000 Watts (approx) Surge Protected

# **Supplied With:**

PDU-12WS-V-SP-1U  12 Way Vertical PDU  
  
Cabinet brackets (Fitted)  
*\* Specifications and product design are subject to change. E&OE.*

Are you looking to protect your valuable Networking, IT or Telco infrastructure from damaging voltage surges? Need a low cost but effective solution for wide scale deployment that prohibits the usage of full scale UPS systems? The new LMS Data SurgePro range of Voltage Surge protected Power Distribution Units (PDU) allow just that sort of protection for your equipment. Featuring the latest in Metal Oxide Varistor (MOV) technology, the SurgePro will block any input voltage surges up to around 4 times the nominal input voltage, meaning your IT Networking Switches, Servers, NAS devices and PBX device s will run for longer and thus reduce system downtime.

# **specifications:**

Voltage Surge Protected Power Distribution

MOV (metal oxide varistor) Surge technology

TSD (transient suppression diode) Spike prevention

Surge system LED confirmation

Standard vertical design for Enclosure fitment

Standard UK type sockets; rated 13A; 12 Way

Protected neon On/Off Switch

Generous 1.8 approx. metre high-load UK cable