### Re-Wireable Male Inline Plug 16 Amps @ 250V - Commando (PWR-CMD-P1234)



# **Description:**

# The LMS Power **PWR-CMD-P1234**is a high quality, IP44 rated and completelyre-wireable 16 Amp Commando plug used for very high electrical load applications.The standard design used for power generation, power distribution extensions and other appliances that need the larger 16 Amp conformance standard.Quality build assured, 16 Amp rated nickel pole design together with a large cable entry cross-section.

# **Key Features:**

Standardised Commando Plug

 Rated at up to 16 Amps up to 250 Volts

 Fully re-wireable with screen down terminals

 IP44 Weather proof rating

# **Applications:**

Create bespoke electrical connections electrical systems

Create electrical connections for very high power appliances

Needed when separate electrical circuits are required

# **Product Code:**

Part Number: PWR-CMD-P1234

EAN: 8400800037862

Weight: 0.1Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 2-Year Warranty

Chassis                   Thermoplastic, screw down housing

Load                        16 Amps 250 Volts (Nominal)

Poles/Hours            2P+E/6H

Standards               CE, Intertek Certified

Cable Entry            6mm-12mm (approx)

# **Supplied With:**

PWR-CMD-P1234 Commando Plug

*\* Specifications and product design are subject to change. E&OE.*